**Methodology**

Design is in accordance with the Load and Resistance Factor Design (LRFD) methodology.

Design is in accordance with the Allowable Strength Design (ASD) methodology.

Design is in accordance with the Load Factor Design (LFD) methodology.

Design is in accordance with the Allowable Stress Design (ASD) methodology.